1. DShow
	uvcham.ax must be registered before use. Run the following command in Administrator mode:
		regsvr32 x86\uvcham.ax
		regsvr32 x64\uvcham.ax
	to register the x86 and x64 versions respectively.
	
	
	Supported interfaces:
		Filter:
				IBaseFilter
				ISpecifyPropertyPages
				IAMFilterMiscFlags
				IAMVideoProcAmp
				IVideoProcAmp
				ICameraControl
				IAMCameraControl
				IUvcham (see uvcham_dshow.h)
		
		Output Pin:
				IPin
				IAMStreamConfig
				IKsPropertySet
				ISpecifyPropertyPages
				IAMVideoProcAmp
				IVideoProcAmp
				ICameraControl
				IAMCameraControl
				IUvcham (see uvcham_dshow.h)
	
	
	Output Pin Media Types:
		MEDIATYPE_Video
		MEDIASUBTYPE_RGB24 (always RGB24)
		FORMAT_VideoInfo
	
2. Twain
	Copy x86\uvcham.ds to Windows\twain_32, x64\uvcham.ds to Windows\twain_64, that is all